(footprint "KINGCONN_7TFCN-F0-0126_MicroSD_PushPush" (version 20221018) (generator kingconn_drawing_to_footprint)
  (layer "F.Cu")
  (descr "KINGCONN 7TFCN-F0-0126 micro-SD push-push, H=1.15mm. Land pattern extracted from KINGCONN drawing 7TFCN-F0-0126 rev A and verified against the printed dimensions.")
  (tags "connector micro-sd microsd push-push kingconn")
  (attr smd)
  (fp_text reference "J**" (at 0 -2.2) (layer "F.SilkS"))
  (fp_text value "KINGCONN_7TFCN-F0-0126_MicroSD_PushPush" (at 0 9.90) (layer "F.Fab"))
  (pad "SH" smd rect (at -2.139 0.000) (size 1.397 0.401) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at 2.109 0.000) (size 1.397 0.401) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at -5.298 0.297) (size 1.300 0.996) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at 5.294 0.297) (size 1.300 0.996) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at -5.748 2.658) (size 0.401 1.203) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at 5.747 2.658) (size 0.394 1.203) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at -5.748 5.254) (size 0.401 1.196) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at 5.747 5.254) (size 0.394 1.196) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -3.420 7.016) (size 0.453 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -2.721 7.016) (size 0.453 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -2.020 7.016) (size 0.446 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -1.321 7.016) (size 0.446 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -0.620 7.016) (size 0.453 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 1.078 7.016) (size 0.446 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 1.779 7.016) (size 0.453 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 2.478 7.016) (size 0.453 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at 3.176 7.016) (size 0.453 0.698) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at -5.473 7.553) (size 0.951 1.397) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SH" smd rect (at 5.294 7.553) (size 1.300 1.397) (layers "F.Cu" "F.Paste" "F.Mask"))
)