(kicad_symbol_lib (version 20211014) (generator kingconn)
  (symbol "KINGCONN_7MSDP-F0-0037" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 12.70 0))
    (property "Value" "KINGCONN_7MSDP-F0-0037" (at 0 -12.70 0))
    (property "Footprint" "KingConn:KINGCONN_7MSDP-F0-0037_MicroSD_PushPush" (at 0 0 0))
    (property "Datasheet" "https://kingconn.com.tw/files/7MSDP-F0-0037.pdf" (at 0 0 0))
    (property "Description" "KINGCONN micro-SD push-push, H=1.29mm, card-detect switch" (at 0 0 0))
    (property "Manufacturer" "KINGCONN" (at 0 0 0))
    (symbol "KINGCONN_7MSDP-F0-0037_0_1")
    (symbol "KINGCONN_7MSDP-F0-0037_1_1"
      (pin bidirectional line (at -12.7 7.62 0) (length 5.08) (name "DAT2") (number "1"))
      (pin bidirectional line (at -12.7 5.08 0) (length 5.08) (name "CD/DAT3") (number "2"))
      (pin bidirectional line (at -12.7 2.54 0) (length 5.08) (name "CMD") (number "3"))
      (pin power_in line (at -12.7 0.00 0) (length 5.08) (name "VDD") (number "4"))
      (pin input line (at -12.7 -2.54 0) (length 5.08) (name "CLK") (number "5"))
      (pin power_in line (at -12.7 -5.08 0) (length 5.08) (name "VSS") (number "6"))
      (pin bidirectional line (at 12.7 7.62 180) (length 5.08) (name "DAT0") (number "7"))
      (pin bidirectional line (at 12.7 5.08 180) (length 5.08) (name "DAT1") (number "8"))
      (pin passive line (at 12.7 2.54 180) (length 5.08) (name "CD1_COMMON") (number "10"))
      (pin passive line (at 12.7 0.00 180) (length 5.08) (name "CD2_DETECT") (number "11"))
      (pin passive line (at 12.7 -2.54 180) (length 5.08) (name "SHIELD") (number "9"))
    )
  )
  (symbol "KINGCONN_7TFCN-F0-0126" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 12.70 0))
    (property "Value" "KINGCONN_7TFCN-F0-0126" (at 0 -12.70 0))
    (property "Footprint" "KingConn:KINGCONN_7TFCN-F0-0126_MicroSD_PushPush" (at 0 0 0))
    (property "Datasheet" "https://kingconn.com.tw/files/7TFCN-F0-0126.pdf" (at 0 0 0))
    (property "Description" "KINGCONN micro-SD push-push, H=1.15mm, card-detect" (at 0 0 0))
    (property "Manufacturer" "KINGCONN" (at 0 0 0))
    (symbol "KINGCONN_7TFCN-F0-0126_0_1")
    (symbol "KINGCONN_7TFCN-F0-0126_1_1"
      (pin bidirectional line (at -12.7 7.62 0) (length 5.08) (name "DAT2") (number "1"))
      (pin bidirectional line (at -12.7 5.08 0) (length 5.08) (name "CD/DAT3") (number "2"))
      (pin bidirectional line (at -12.7 2.54 0) (length 5.08) (name "CMD") (number "3"))
      (pin power_in line (at -12.7 0.00 0) (length 5.08) (name "VDD") (number "4"))
      (pin input line (at -12.7 -2.54 0) (length 5.08) (name "CLK") (number "5"))
      (pin power_in line (at -12.7 -5.08 0) (length 5.08) (name "VSS") (number "6"))
      (pin bidirectional line (at 12.7 7.62 180) (length 5.08) (name "DAT0") (number "7"))
      (pin bidirectional line (at 12.7 5.08 180) (length 5.08) (name "DAT1") (number "8"))
      (pin passive line (at 12.7 2.54 180) (length 5.08) (name "CD") (number "9"))
      (pin passive line (at 12.7 0.00 180) (length 5.08) (name "SHIELD") (number "SH"))
    )
  )
  (symbol "KINGCONN_7MSDP-AA-1110" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 12.70 0))
    (property "Value" "KINGCONN_7MSDP-AA-1110" (at 0 -12.70 0))
    (property "Footprint" "KingConn:KINGCONN_7MSDP-AA-1110_MicroSD_PushPush_Reverse" (at 0 0 0))
    (property "Datasheet" "https://kingconn.com.tw/files/7MSDP-AA-1110-B.pdf" (at 0 0 0))
    (property "Description" "KINGCONN micro-SD push-push REVERSE type; pin names follow the standard microSD assignment (drawing numbers pins only)" (at 0 0 0))
    (property "Manufacturer" "KINGCONN" (at 0 0 0))
    (symbol "KINGCONN_7MSDP-AA-1110_0_1")
    (symbol "KINGCONN_7MSDP-AA-1110_1_1"
      (pin bidirectional line (at -12.7 7.62 0) (length 5.08) (name "DAT2") (number "1"))
      (pin bidirectional line (at -12.7 5.08 0) (length 5.08) (name "CD/DAT3") (number "2"))
      (pin bidirectional line (at -12.7 2.54 0) (length 5.08) (name "CMD") (number "3"))
      (pin power_in line (at -12.7 0.00 0) (length 5.08) (name "VDD") (number "4"))
      (pin input line (at -12.7 -2.54 0) (length 5.08) (name "CLK") (number "5"))
      (pin power_in line (at -12.7 -5.08 0) (length 5.08) (name "VSS") (number "6"))
      (pin bidirectional line (at 12.7 7.62 180) (length 5.08) (name "DAT0") (number "7"))
      (pin bidirectional line (at 12.7 5.08 180) (length 5.08) (name "DAT1") (number "8"))
      (pin passive line (at 12.7 2.54 180) (length 5.08) (name "DET_SW1") (number "SW1"))
      (pin passive line (at 12.7 0.00 180) (length 5.08) (name "DET_SW2") (number "SW2"))
      (pin passive line (at 12.7 -2.54 180) (length 5.08) (name "SHIELD") (number "SH"))
    )
  )
  (symbol "KINGCONN_7MSDP-FA-0024" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 12.70 0))
    (property "Value" "KINGCONN_7MSDP-FA-0024" (at 0 -12.70 0))
    (property "Footprint" "KingConn:KINGCONN_7MSDP-FA-0024_MicroSD_PushPush" (at 0 0 0))
    (property "Datasheet" "https://kingconn.com.tw/files/7MSDP-FA-0024.pdf" (at 0 0 0))
    (property "Description" "KINGCONN micro-SD push-push, H=1.28mm, detect switch DSW1/DSW2" (at 0 0 0))
    (property "Manufacturer" "KINGCONN" (at 0 0 0))
    (symbol "KINGCONN_7MSDP-FA-0024_0_1")
    (symbol "KINGCONN_7MSDP-FA-0024_1_1"
      (pin bidirectional line (at -12.7 7.62 0) (length 5.08) (name "DAT2") (number "1"))
      (pin bidirectional line (at -12.7 5.08 0) (length 5.08) (name "CD/DAT3") (number "2"))
      (pin bidirectional line (at -12.7 2.54 0) (length 5.08) (name "CMD") (number "3"))
      (pin power_in line (at -12.7 0.00 0) (length 5.08) (name "VDD") (number "4"))
      (pin input line (at -12.7 -2.54 0) (length 5.08) (name "CLK") (number "5"))
      (pin power_in line (at -12.7 -5.08 0) (length 5.08) (name "VSS") (number "6"))
      (pin bidirectional line (at 12.7 7.62 180) (length 5.08) (name "DAT0") (number "7"))
      (pin bidirectional line (at 12.7 5.08 180) (length 5.08) (name "DAT1") (number "8"))
      (pin passive line (at 12.7 2.54 180) (length 5.08) (name "DET_SW1") (number "DSW1"))
      (pin passive line (at 12.7 0.00 180) (length 5.08) (name "DET_SW2") (number "DSW2"))
      (pin passive line (at 12.7 -2.54 180) (length 5.08) (name "SHIELD") (number "SH"))
    )
  )
)